Denver Elections Division

Acceptance testing procedures for Dominion Democracy Suite 4.21

**Acceptance Testing for Dominion EMS Admin Machine/Server**

* Unpack, connect, power on equipment, and inspect for damage.
* Load a test election into EED and produce ballot PDFs and election files.
* Start RTR services.
* Start Adjudication admin services on server

After Scanning is complete:

* Submit batches to RTR from Adjudication Admin client.
* Produce results reports and compare against expected results.

**Acceptance Testing for Dominion ICX Ballot Marking Devices**

* Unpack equipment and inspect for visual damage.
* Connect and power on equipment according to ICX guide from Dominion.
* Load an election files onto each ICX server according to ICX guide from Dominion.
* Activate 5 voting sessions for each ICX and vote the ballots according to the standard pattern, 1,2,2,3,3,3 etc.
* Activate and additional session and vote on each accessible ICX device to ensure the ADA capabilities are functioning.

**Acceptance Testing for Dominion ICC Scanners**

* Unpack, connect, and power on equipment according to ICC guide from Dominion and inspect for damage.
* Configure ICC application to write files to the results folder in the NAS on the server for the current test project.
* Scan a pre-marked ballot deck with the standard pattern including exception ballots.
* Scan the ICX ballots that were produced during the ICX acceptance testing.

**Acceptance Testing for Dominion Adjudication Clients**

* Unpack, connect, power on equipment, and inspect for damage.
* Start adjudication client services.
* Adjudicate ballots.